iButton2 Configuration Utility V1.0.0

=========================================
Device FW: Must "1BT2-013 or 1BT2-102" later
OS: Vista ,Windows 7/8/10

* Release Note:
V1.0.0  (2017/09/12)
    1.Add new import CFG function can set all attributes then change interface, need 1BT2-013 or 1BT2-102 later can support.

V0.9.9  (2017/06/15)
    1.Modify check function to support firmware "1BT2-101" or later, PID = F108

V0.9.8  (2017/04/07)
    1.Only support firmware "1BT2-100" version
    2.PreAmble, PostAmble, Remove Data can input hex number

V0.9.7  (2017/03/15)
    1.Add "Import/Export" and "Default" setting file function
    2.Add "Remove ID Code" function

V0.9.6A  (2014/09/25)
    1.Release firmware update tool "nuc100Writer" V1.0.2.0
    2.Firmware update tool add "RECONNIBT" mode to fix update missing then IButton blocked issue

V0.9.6  (2014/09/25)
    1. Fix Set PreAmble, PostAmble, Remove Data lost Character issue

V0.9.5  (2013/08/13)
	1. Add more code page support(see *Support Code Page)

V0.9.4  (2013/07/23) 
	1. Fix over 0x7F ascii number display fail issue
	2. Add auto detect VCOM number function
	3. Change to OEM version

V0.9.3	(2012/11/26) *V0.9.3 
	1. Add USB key board country setting
	2. Add control code input function
	3. Add F/W update function(FW update tool V1.0.1.0)
	4. Fix some connect fail bug
	
V0.9.0  (2012/10/09)
	1. Initial version
	2. Support iButton RS-232 and USB KB interface


*Support Code Page

Name    		OEM Page Number
==========================================
Big5			950
Big5-HKSCS		950
CP949			949
CP437			437
IBM 850			850
IBM 866			866
IBM 874			874
Windows-1250 - 1258	1250 - 1258
EUC-JP			20932,51932
EUC-KR			51949
GB18030-0		54936
ISO 2022-JP		50220,50221,50222
ISO 8859-1 to 10	28591-28599
ISO 8859-13             28603
ISO 8859-15             28605
JIS X 0201		50222
JIS X 0208		20932
KOI8-R			20866
KOI8-U			21866
Shift-JIS		932
UTF-8			65001
UTF-16,UTF-16LE		1200
UTF-16BE		1201
UTF-32,UTF-32LE		12000
UTF-32BE		12001